// Hud modes setup
   mando_hud_init_code = {
                [0.42,0.89,0.20, true]execVm"mando_missiles\huds\custom\custom_radar.sqf";
				[]execVm"mando_missiles\huds\custom\custom_hud_ils.sqf";
   };

   mando_hud_modes = [];

   mando_hud_modes = mando_hud_modes + [[
   11,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_
   1,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["Air"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0.17,	// Aim circle diameter
   "Air - AIM9", // HUD Text
   0.015,        // IR accuracy for headon shots or radar accuracy for ECM targets
   6,		// Number of simultaneously detected HUD targets (max is 6)
   1000, 	// Sensor width / 2 in meters
   5000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];

   mando_hud_modes = mando_hud_modes + [[
   12,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_
   1,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["Air"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0.17,	// Aim circle diameter
   "Air - AIM9", // HUD Text
   0.015,        // IR accuracy for headon shots or radar accuracy for ECM targets
   6,		// Number of simultaneously detected HUD targets (max is 6)
   1000, 	// Sensor width / 2 in meters
   5000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];


   mando_hud_modes = mando_hud_modes + [[
   13,
   false,
   0,
   ["Air"],
   0.19,
   "Air - AIM120",
   0.03,        // IR accuracy for headon shots or radar accuracy for ECM targets
   6,		// Number of simultaneously detected HUD targets (max is 6)
   1000, 	// Sensor width / 2 in meters
   10000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];


   mando_hud_modes = mando_hud_modes + [[
   14,
   false,
   0,
   ["Air"],
   0.19,
   "Air - AIM120",
   0.03,        // IR accuracy for headon shots or radar accuracy for ECM targets
   6,		// Number of simultaneously detected HUD targets (max is 6)
   1000, 	// Sensor width / 2 in meters
   10000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];

   mando_hud_modes = mando_hud_modes + [[
   15,
   false,
   0,
   ["Air"],
   0.19,
   "Air - AIM120",
   0.03,        // IR accuracy for headon shots or radar accuracy for ECM targets
   6,		// Number of simultaneously detected HUD targets (max is 6)
   1000, 	// Sensor width / 2 in meters
   10000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];

   mando_hud_modes = mando_hud_modes + [[
   16,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_ ?
   4,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["LOCATIONS"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0,	// Aim circle diameter
   "CCIP/Nav CBU", // HUD Text
   0.015,       // IR accuracy for headon shots or radar accuracy with ECM
   6,		// Number of simultaneously detected HUD targets (max is 6)
   800, 	// Sensor width / 2 in meters
   3000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];

   mando_hud_modes = mando_hud_modes + [[
   17,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_ ?
   4,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["LOCATIONS"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0,	// Aim circle diameter
   "CCIP/Nav Mk82", // HUD Text
   0.015,       // IR accuracy for headon shots or radar accuracy with ECM
   6,		// Number of simultaneously detected HUD targets (max is 6)
   800, 	// Sensor width / 2 in meters
   3000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];

   mando_hud_modes = mando_hud_modes + [[
   18,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_ ?
   4,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["LOCATIONS"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0,	// Aim circle diameter
   "CCIP/Nav Mk84", // HUD Text
   0.015,       // IR accuracy for headon shots or radar accuracy with ECM
   6,		// Number of simultaneously detected HUD targets (max is 6)
   800, 	// Sensor width / 2 in meters
   3000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];


   mando_hud_modes = mando_hud_modes + [[
   -1,		// Missile to be used
   false,	// Keep coords set in mando_assignvehicle_by_ ?
   1,           // Guidance type 0 Radar, 1 IR, 2 SARH, 3 Manual
   ["LOCATIONS"],     // Type of targets ["Air"], [""LandVehicle"], ["RADAR"], ["REMOTE"] or ["GROUND"]
   0,	// Aim circle diameter
   "Navigation", // HUD Text
   0.015,       // IR accuracy for headon shots or radar accuracy with ECM
   6,		// Number of simultaneously detected HUD targets (max is 6)
   800, 	// Sensor width / 2 in meters
   3000,	// Sensor length / 2 in meters
   3            // Normal time to lock
   ]];


   mando_hud_num_modes = count mando_hud_modes; // Number of available modes

// Missile parameters setup
   call compile (preprocessFileLineNumbers (mando_missile_path+"huds\mando_hud_RKT_miss_params.sqf"));